### DM LPG DISPENSER TYPE ROOF/MULTIMEDIA

The roof type dispenser is designed to be minimally affected by the weather due to roof protection. . Its simple and elegant appearance is highly preferred and widely used. With its fast and practical system, it offers high capacity filling. Ergonomically designed and maximum sealed. We can produce the machine is with single, double and four nozzles and low-height electronic panel. In production, stainless steel and electrolysis coating is resistant to weather conditions and corrosion.

We can produce the machines with different dimensions and features.

Optional mass flow meter is also available. Mass flow meters are compatible with each DM LPG Dispenser model. Can be 1-2 filling guns.

DM LPG Dispenser type Roof/Multipedia colorizes your station with the new 21.5" full HD LED (1920\*1080) 1000 nits LCD Panel.

**Technicality**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | **DM-DISRM-M01** | **DM-DISRM-M02** | **DM-DISRM-M04** |
| Grades |  | 1 | 1 | 1 |
| No of nozzles |  | 1 | 2 | 4 |
| Simultaneous fillings |  | 1 | 2 | 4 |
| Meter Type |  | Mechanic | Mechanic | Mechanic |
| Capacity Max. | Lt/Min (kg/min) | 50 ( 27,5 ) | 50 ( 27,5 ) | 50 ( 27,5 ) |
| Capacity Min. | Lt/Min (kg/min) | 5 ( 2,75 ) | 5 ( 2,75 ) | 5 ( 2,75 ) |
| Hose (4.2 m) | INCH | 1/2" | 1/2" | 1/2" |
| Operating Temperature | (°C) | -25+55 | -25+55 | -25+55 |
| Relative humidity | (%) | 100 | 100 | 100 |
| Supply voltage | (V) | 230 | 230 | 230 |
| Frequency | (Hz) | 50 | 50 | 50 |
| Electronic units power | (W) | 100 | 100 | 100 |
| **Dimensions (W x L x H)** | (mm) | 900 x 500 x 2000 | 900 x 500 x 2000 | 900 x 550 x 2050 |
| **Weight** | (Kg) | 150 | 190 | 270 |
| Amount/Volume programming |  | money/liter | money/liter | money/liter |
| Emergency stop |  | 1 | 2 | 2 |
| Sight glass |  | NO | NO | NO |
| Nozzle swivel |  | YES | YES | YES |
| Breakaway coupling |  | 3/4" | 3/4" | 3/4" |
| Filter |  | YES | YES | YES |
| Manometer |  | YES | YES | YES |
|  |  | **DM-DISRD-M01** | **DM-DISRD-M02** |  |
| Grades |  | 1 | 1 |  |
| No of nozzles |  | 1 | 2 |  |
| Simultaneous fillings |  | 1 | 2 |  |
| Meter Type |  | Mass Flow | Mass Flow |  |
| Capacity Max. | (kg/h) | 6500 | 6500 |  |
| Capacity Min. | (kg/h) | 0 | 0 |  |
| Hose (4.2 m) | INCH | 1/2" | 1/2" |  |
| Operating Temperature | (°C) | -25+55 | -25+55 |  |
| Relative humidity | (%) | 100 | 100 |  |
| Supply voltage | (V) | 230 | 230 |  |
| Frequency | (Hz) | 50 | 50 |  |
| Electronic units power | (W) | 100 | 100 |  |
| **Dimensions (W x L x H)** | (mm) | 900 x 500 x 2000 | 900 x 500 x 2000 |  |
| **Weight** | (Kg) | 150 | 190 |  |
| Amount/Volume programming |  | money/liter | money/liter |  |
| Emergency stop |  | 1 | 2 |  |
| Sight glass |  | NO | NO |  |
| Nozzle swivel |  | YES | YES |  |
| Breakaway coupling |  | 3/4" | 3/4" |  |
| Filter |  | YES | YES |  |
| Manometer |  | YES | YES |  |





**NOW, THE NEWEST DM LPG DISPENSERS**

**TYPE ROOF/MULTIMEDIA**



**PRODUCT CODE: DM-DISRX-M04**

2 Separator - 4 Meter

4 Nozzle - 4 Display – 4 Keypad